|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **ANNEXURE - 1** | | | | | | | | |
| **Sr No** | **REQUIRE ARCHIVAL CORRUGATED BOXES** | **To be filled by Vendors** | | | | | | |
|  | **Dimensions + Total No of Box required** | **Availability** | | | **Rate per unit** | **Total cost** | | **Cost with Taxes** |
| **Yes** | **No** | |
| 1 | **Box Dimensions** |  |  | |  |  | |  |
|  | 22" x 151/2" x 21/2 "  Total No of boxes required: 232 |  |  | |  |  | |  |
| 2 | **Box Dimensions** |  |  | |  |  | |  |
|  | 33" x 22" x 3"  Total No of boxes required: 10 |  |  | |  |  | |  |
| 3 | **Box Dimensions** |  |  | |  |  | |  |
|  | 11" x 8" x 3"  Total No of boxes required: 84 |  |  | |  |  | |  |
|  | **TOTAL AMOUNT (RS.)** |  |  | |  |  | |  |
|  | | | | | | | | |
| Each Box should be manufactured to the following specifications and must present the quality certifications mentioned below. | | | | | | | | |
| **Sr No** | **Specifications** | | | **To be filled by Vendors** | | | | |
| **A** | **Box description and Features** | | | **Availability** | | | | |
| **Yes** | | | **No** | |
| 1 | Archival quality Corrugated board used in fabrication for storage of paper works | | |  | | |  | |
| 2 | Duralong wave Archival Micro corrugated board Drop spine box or Heritage Clamshell type corrugated box | | |  | | |  | |
| 3 | Conservation quality heritage corrugated board to be used as material | | |  | | |  | |
| 4 | The boxes should have a one piece construction where the cover folds back and the box opens flat | | |  | | |  | |
| 5 | Boxes should be shipped flat and be easily assembled without requiring tape or adhesive | | |  | | |  | |
| 6 | Ideal for storage of photographs, archival materials and various objects | | |  | | |  | |
| 7 | Assembly instructions should be provided | | |  | | |  | |

|  |  |  |  |
| --- | --- | --- | --- |
| **Sr No** | **Specifications** | **To be filled by Vendors** | |
| **B** | **Technical Specification for Material used in Boxes** | **Specifications** | |
| **Yes** | **No** |
| 1 | 100% alpha cellulose |  |  |
| 2 | Without the use of recycled or wooden fibres and lignin free |  |  |
| 3 | No optical brighteners |  |  |
| 4 | Acid Free |  |  |
| 5 | Alkaline reserve (buffer) Calcium Carbonate |  |  |
| 6 | pH greater than 8 |  |  |
| 7 | Constructed with E flute corrugated or Duralong wave micro corrugated board (please specify quality) |  |  |
| 8 | Thickness of corrugated board should be 1.6 mm or 1.7mm |  |  |
| 9 | Treated with Fungicide to combat the proliferation of moulds and fungi |  |  |
| **C** | **Certifications** |  |  |
| 1 | ISO 9706 - Permanency requirements for paper |  |  |
| 2 | ANSI / NISO Z.39.48-1992 Permanence for paper in Library and Archives |  |  |
| 3 | Photo Activity Test passed (PAT test) |  |  |
| 4 | ANSI IT 9.16 / ISO 14523-1999 (PAT test) or  ISO 18916 (PAT test) |  |  |