|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Requirements details** | **QTY****(pcs)** | **Rate per unit INR** | **Total cost****(A)****INR** | **Taxes****(B)****INR** | **TOTAL (A + B) INR** |
| **1**a  | Museum Vac®800-watt model with variable controllerCode No 561-1990Dimensions 457 x 241 x 190mm**Specifications**Power Supply 230 Volt model HEPA filter bagsPower Consumption 800 wattAir Flow 30 litres per secondSuction 1400mm H²OCapacity 2.7 litresWeight 5.5kg | 01 |   |   |   |  |
| 1b | Mini Adapter Kit Code No 875-UV-2/1 | 01 |  |  |  |  |
| 1c | HEPA Filter Bags (Grade E10-E11)and Seal Label for P561-1990Museum VacCode No 561-4150 | 20 |  |  |  |  |
| **2**  | Easy-Log USB Temperature and Relative Humidity Datalogger with Calibration CertificateModel No: EL-USB-2-LCD**Specifications**Calibration certificateBattery ½ AAWall mount clipTemperature measurement range: -35 to +80°CRelative Humidity measurement range: 0 to 100%Logging Rate between 10 seconds and 12 hours | 10 |  |  |  |  |
| **Sr. No.** | **Requirements details** | **QTY****(pcs)** | **Rate per unit INR** | **Total cost****(A)****INR** | **Taxes****(B)****INR** | **TOTAL (A + B) INR** |
| **3** | Leica A60FStereo Microscope Flex Arm**Specifications**Flex arm stand - 6:1 zoom ratioZoom range: 5x-30xWorking distance – 122 mm,Ergonomic 38° viewing angle - Max. 46 mm field of view2x 10x/23 high eye point eyepieces with adjustable diopters and eyecupsLED ring light designed focus lens for homogeneous and bright illumination,5600K colour temperature - Diffusor to reduce reflections (removable)Universal power supply, 100V-240V - Inclinable focus arm with 50mm travel range, incl. flex arm stand | 01 |   |   |   |  |
| **4** | Leica Flexacam C3 12 MP camera**Specifications**Sensor type: CMOSSensor size: 1 / 2.3“Sensor format: H: 4,000; V: 3,000 (12 MP)Data interface: USB 3.1 type CMechanical interface: C-mountBit depth / Colour depth: 8-bit | 01 |  |  |  |  |
| **5** | Leica LAX software**Specifications**Compatible with Leica S8APO stereomicroscope | 01 |  |  |  |  |
| **Sr. No.** | **Requirements details** | **QTY****(pcs)** | **Rate per unit INR** | **Total cost****(A)****INR** | **Taxes****(B)****INR** | **TOTAL (A + B) INR** |
| **6**  | Water Demineraliser MOD. MINIDEM 30with mixed-bed ion-exchange resins, to provide high purity water with no salts**Specifications**Power Supply :200V-50Hz single –phase-12V(conductivity meter)Feedwater pressure:5 bar max.Flow rate:420 l/h.max.Ion-exchange resin quantity :30 lApproximate water treatment capacity:-4000lat 20° F 2800l at 30° F-2500l at 34° FWater purity :1 µS/cm | 01 |   |   |   |  |
| **7** | Motorised Ceiling Hanging Drying Rack with adjustable height up to 1.80m from the ceiling with the remote controller.Max Dimension- 1600 x 560mm**Specifications**Max load 35Kg of textilesMaximum descent from the ceiling :180cm | 01 |  |  |  |  |
|  | **Total** |  |
|  | **Shipping with Taxes** |  |
|  | **Gross Total** |  |
|  | **Estimated time of delivery**  |

 Authorised signatory

 Signature and company seal