|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Requirements details** | **QTY**  **(pcs)** | **Rate per unit INR** | **Total cost**  **(A)**  **INR** | **Taxes**  **(B)**  **INR** | **TOTAL (A + B) INR** |
| **1**a | Museum Vac®800-watt model with variable controller  Code No 561-1990  Dimensions  457 x 241 x 190mm  **Specifications**  Power Supply 230 Volt model  HEPA filter bags  Power Consumption 800 watt  Air Flow 30 litres per second  Suction 1400mm H²O  Capacity 2.7 litres  Weight 5.5kg | 01 |  |  |  |  |
| 1b | Mini Adapter Kit  Code No 875-UV-2/1 | 01 |  |  |  |  |
| 1c | HEPA Filter Bags (Grade E10-E11)and Seal Label for P561-1990  Museum Vac  Code No 561-4150 | 20 |  |  |  |  |
| **2** | Easy-Log USB Temperature and Relative Humidity Datalogger with Calibration Certificate  Model No: EL-USB-2-LCD  **Specifications**  Calibration certificate  Battery ½ AA  Wall mount clip  Temperature measurement range: -35 to +80°C  Relative Humidity measurement range: 0 to 100%  Logging Rate between 10 seconds and 12 hours | 10 |  |  |  |  |
| **Sr. No.** | **Requirements details** | **QTY**  **(pcs)** | **Rate per unit INR** | **Total cost**  **(A)**  **INR** | **Taxes**  **(B)**  **INR** | **TOTAL (A + B) INR** |
| **3** | Leica A60FStereo Microscope Flex Arm  **Specifications**  Flex arm stand - 6:1 zoom ratio  Zoom range: 5x-30x  Working distance – 122 mm,  Ergonomic 38° viewing angle - Max. 46 mm field of view  2x 10x/23 high eye point eyepieces with adjustable diopters and eyecups  LED ring light designed focus lens for homogeneous and bright illumination,5600K colour temperature - Diffusor to reduce reflections (removable)  Universal power supply, 100V-240V - Inclinable focus arm with 50mm travel range, incl. flex arm stand | 01 |  |  |  |  |
| **4** | Leica Flexacam C3 12 MP camera  **Specifications**  Sensor type: CMOS  Sensor size: 1 / 2.3“  Sensor format: H: 4,000; V: 3,000 (12 MP)  Data interface: USB 3.1 type C  Mechanical interface: C-mount  Bit depth / Colour depth: 8-bit | 01 |  |  |  |  |
| **5** | Leica LAX software  **Specifications**  Compatible with Leica S8APO stereomicroscope | 01 |  |  |  |  |
| **Sr. No.** | **Requirements details** | **QTY**  **(pcs)** | **Rate per unit INR** | **Total cost**  **(A)**  **INR** | **Taxes**  **(B)**  **INR** | **TOTAL (A + B) INR** |
| **6** | Water Demineraliser  MOD. MINIDEM 30  with mixed-bed ion-exchange resins, to provide high purity water with no salts  **Specifications**  Power Supply :200V-50Hz single –phase-12V(conductivity meter)  Feedwater pressure:5 bar max.  Flow rate:420 l/h.max.  Ion-exchange resin quantity :30 l  Approximate water treatment capacity:-4000lat 20° F 2800l at 30° F-2500l at 34° F  Water purity :1 µS/cm | 01 |  |  |  |  |
| **7** | Motorised Ceiling Hanging Drying Rack with adjustable height up to 1.80m from the ceiling with the remote controller.  Max Dimension-  1600 x 560mm  **Specifications**  Max load 35Kg of textiles  Maximum descent from the ceiling :180cm | 01 |  |  |  |  |
|  | **Total** | | | | |  |
|  | **Shipping with Taxes** | | | | |  |
|  | **Gross Total** | | | | |  |
|  | **Estimated time of delivery** | | | | | |

Authorised signatory

Signature and company seal