Chhatrapati Shivaji Maharaj Vastu Sangrahalaya  
159-161 Mahatma Gandhi Road,  
Fort, Mumbai - 400023  
Maharashtra, India

EOI No.CSMVS/**E059**/2019-20 May 6, 2019

**TENDER NOTICE - E059**

**Landscape Lighting Electrical Work**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **NO** | **UNIT** | **DESCRIPTION** | **QTY** | **RATE** | **AMOUNT** |
|  |  |  |  |  |  |
| **1.0** |  | **LIGHT FITTINGS** |  |  |  |
|  |  |  |  |  |  |
| 1.1 |  | Supply and or installation, testing and commissioing |  |  |  |
|  |  | of landscape light fitting as specified and shown on |  |  |  |
|  |  | drawings complete with |  |  |  |
|  |  |  |  |  |  |
|  |  | a) Fixing, mounting accessories |  |  |  |
|  |  | b) Foundation wherever required |  |  |  |
|  |  | c) Earthing |  |  |  |
|  |  |  |  |  |  |
| 1.1.1 | Each | Installation of bollard light fitting | 42 |  |  |
|  |  |  |  |  |  |
| 1.1.2 | Each | Installation of 30W LED ground mounted flood light | 14 |  |  |
|  |  | with antiglare film, K-LITE 7071, 4000 K & built in driver |  |  |  |
|  |  |  |  |  |  |
| 1.1.3 | Each | Installation of 30W LED tree mounted uplighter flood | 12 |  |  |
|  |  | light with antiglare film, K-LITE 7071 & built-in driver |  |  |  |
|  |  |  |  |  |  |
| 1.1.4 | Set | Installation of Flexible, IP-67, 6W/M LED strip, mounted | 12 |  |  |
|  |  | horizontal below bench not more than 2M long, K-LITE, |  |  |  |
|  |  | 3000 complete with mounting clips |  |  |  |
|  |  |  |  |  |  |
| 1.1.5 | Set | Installation of Flexible, IP-67, 6W/M LED strip, mounted | 22 |  |  |
|  |  | vertical on seat support not more than 1M long, K-LITE, |  |  |  |
|  |  | 3000K complete with mounting clips |  |  |  |
|  |  |  |  |  |  |
| 1.1.6 | Each | Supply and installation of ground buried IP 68 HENSEL | 8 |  |  |
|  |  | weather proof box with 60W 12V DG power unit (driver) |  |  |  |
|  |  |  |  |  |  |
| 1.1.7 | Metre | Supply and laying of 2C-2.5 sq.m flexible copper | 150 |  |  |
|  |  | cable between driver & LED strip with necessary |  |  |  |
|  |  |  |  |  |  |
| 1.1.8 | Metre | Supply and laying of 3C-2.5 sq.m flexible copper cable | 350 |  |  |
|  |  | between JB and ground / tree lighter with clamps /nylon |  |  |  |
|  |  | ties wherever connector required |  |  |  |
|  |  |  |  |  |  |
| 1.1.9 | Each | Supply and providing of ground buried IP 68 HENSEL | 20 |  |  |
|  |  | weather proof box with 10 way, 10A terminal strips |  |  |  |
|  |  |  |  |  |  |
| 1.1.10 | Each | Supply and providing of 2C / 3C - 2.5 Cable termination | 80 |  |  |
|  |  | using lugs and nylon glands |  |  |  |
|  |  |  |  |  |  |
| 1.1.11 | Metre | Supply and laying of 3C -2.5 2XWY (Copper armoured) | 400 |  |  |
|  |  | FRLS cables in ground / tree etc. including excavation / |  |  |  |
|  |  | back filling, brick protection, sand bed etc. |  |  |  |
|  |  |  |  |  |  |
| 1.1.12 | Each | Supply and providing of 3C - 2.5 sq.mm cable termination | 20 |  |  |
|  |  | with double compression glands |  |  |  |
|  |  |  |  |  |  |
| 1.1.13 | Each | Supply and providing of 6A,switch in weather proof | 6 |  |  |
|  |  | PLEXO of LEGRAND |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  | TOTAL |  |  |  |

Tenderers are requested to submit their Tender along with their company profile. Superscribe the envelope with **“E059 – Landscape Lighting Electrical Work”** to Assistant Director (Administration) on the above-mentioned address latest by 13th May 2019 upto 4:00 p.m.

CSMVS reserves all the rights in the selection process.